SYSTEM DE0_NANO_SOPC
{
   # 
   # Generated by: com.altera.sopcmodel.ensemble.EnsembleGeneratePTF
   # Date: 2011.02.21.20:20:32
   # 
   #    clock_source "clk_50"
   #    altera_nios2 "cpu"
   #    altera_avalon_jtag_uart "jtag_uart"
   #    altera_avalon_onchip_memory2 "onchip_memory2"
   #    altera_avalon_pio "pio_led"
   # 
   #    Contains 11 connections.
   # 
   System_Wizard_Version = "8.0";
   Builder_Application = "sopc_builder_ca";
   #. values for Builder_Application are:
   #.    sopc_builder_preview --> 6.1p, 7.0p prerelease versions
   #.    sopc_builder_ca      --> 7.1 and later
   #.    (missing) --> 6.0 or earlier
   WIZARD_SCRIPT_ARGUMENTS 
   {
      hdl_language = "verilog";
      device_family = "CYCLONEIVE";
      device_family_id = "CYCLONEIVE";
      generate_sdk = "0";
      do_build_sim = "0";
      hardcopy_compatible = "0";
      CLOCKS 
      {
         CLOCK clk_50
         {
            frequency = "50000000";
            source = "External";
            Is_Clock_Source = "0";
            display_name = "clk_50";
            pipeline = "0";
            clock_module_connection_point_for_c2h = "clk_50.clk";
         }
      }
   }
   MODULE cpu
   {
      MASTER instruction_master
      {
         PORT_WIRING 
         {
            PORT clk
            {
               type = "clk";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT reset_n
            {
               type = "reset_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT i_address
            {
               type = "address";
               width = "17";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT i_read
            {
               type = "read";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT i_readdata
            {
               type = "readdata";
               width = "32";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT i_readdatavalid
            {
               type = "readdatavalid";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT i_waitrequest
            {
               type = "waitrequest";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT jtag_debug_module_resetrequest
            {
               type = "resetrequest";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Is_Asynchronous = "0";
            DBS_Big_Endian = "0";
            Adapts_To = "";
            Do_Stream_Reads = "0";
            Do_Stream_Writes = "0";
            Max_Address_Width = "32";
            Data_Width = "32";
            Address_Width = "17";
            Maximum_Burst_Size = "1";
            Register_Incoming_Signals = "0";
            Register_Outgoing_Signals = "0";
            Interleave_Bursts = "0";
            Linewrap_Bursts = "0";
            Burst_On_Burst_Boundaries_Only = "0";
            Always_Burst_Max_Burst = "0";
            Is_Big_Endian = "0";
            Is_Enabled = "1";
            Is_Instruction_Master = "1";
         }
         MEMORY_MAP 
         {
            Entry cpu/jtag_debug_module
            {
               address = "0x00010800";
               span = "0x00000800";
               is_bridge = "0";
            }
            Entry onchip_memory2/s1
            {
               address = "0x00008000";
               span = "0x00006590";
               is_bridge = "0";
            }
         }
      }
      MASTER custom_instruction_master
      {
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "nios_custom_instruction";
            Data_Width = "32";
            Address_Width = "8";
            Is_Custom_Instruction = "1";
            Is_Enabled = "0";
            Max_Address_Width = "8";
         }
         PORT_WIRING 
         {
            PORT dataa
            {
               type = "dataa";
               width = "32";
               direction = "output";
            }
            PORT datab
            {
               type = "datab";
               width = "32";
               direction = "output";
            }
            PORT result
            {
               type = "result";
               width = "32";
               direction = "input";
            }
            PORT clk_en
            {
               type = "clk_en";
               width = "1";
               direction = "output";
            }
            PORT reset
            {
               type = "reset";
               width = "1";
               direction = "output";
            }
            PORT start
            {
               type = "start";
               width = "1";
               direction = "output";
            }
            PORT done
            {
               type = "done";
               width = "1";
               direction = "input";
            }
            PORT n
            {
               type = "n";
               width = "8";
               direction = "output";
            }
            PORT a
            {
               type = "a";
               width = "5";
               direction = "output";
            }
            PORT b
            {
               type = "b";
               width = "5";
               direction = "output";
            }
            PORT c
            {
               type = "c";
               width = "5";
               direction = "output";
            }
            PORT readra
            {
               type = "readra";
               width = "1";
               direction = "output";
            }
            PORT readrb
            {
               type = "readrb";
               width = "1";
               direction = "output";
            }
            PORT writerc
            {
               type = "writerc";
               width = "1";
               direction = "output";
            }
         }
      }
      SLAVE jtag_debug_module
      {
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Write_Wait_States = "0cycles";
            Read_Wait_States = "1cycles";
            Hold_Time = "0cycles";
            Setup_Time = "0cycles";
            Is_Printable_Device = "0";
            Address_Alignment = "dynamic";
            Well_Behaved_Waitrequest = "0";
            Is_Nonvolatile_Storage = "0";
            Address_Span = "2048";
            Read_Latency = "0";
            Is_Memory_Device = "1";
            Maximum_Pending_Read_Transactions = "0";
            Minimum_Uninterrupted_Run_Length = "1";
            Accepts_Internal_Connections = "1";
            Write_Latency = "0";
            Is_Flash = "0";
            Data_Width = "32";
            Address_Width = "9";
            Maximum_Burst_Size = "1";
            Register_Incoming_Signals = "0";
            Register_Outgoing_Signals = "0";
            Interleave_Bursts = "0";
            Linewrap_Bursts = "0";
            Burst_On_Burst_Boundaries_Only = "0";
            Always_Burst_Max_Burst = "0";
            Is_Big_Endian = "0";
            Is_Enabled = "1";
            Accepts_External_Connections = "1";
            Requires_Internal_Connections = "";
            MASTERED_BY cpu/instruction_master
            {
               priority = "1";
               Offset_Address = "0x00010800";
            }
            MASTERED_BY cpu/data_master
            {
               priority = "1";
               Offset_Address = "0x00010800";
            }
            Base_Address = "0x00010800";
         }
         PORT_WIRING 
         {
            PORT jtag_debug_module_address
            {
               type = "address";
               width = "9";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT jtag_debug_module_begintransfer
            {
               type = "begintransfer";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT jtag_debug_module_byteenable
            {
               type = "byteenable";
               width = "4";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT jtag_debug_module_debugaccess
            {
               type = "debugaccess";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT jtag_debug_module_readdata
            {
               type = "readdata";
               width = "32";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT jtag_debug_module_select
            {
               type = "chipselect";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT jtag_debug_module_write
            {
               type = "write";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT jtag_debug_module_writedata
            {
               type = "writedata";
               width = "32";
               direction = "input";
               Is_Enabled = "1";
            }
         }
      }
      MASTER data_master
      {
         SYSTEM_BUILDER_INFO 
         {
            Has_IRQ = "1";
            Irq_Scheme = "individual_requests";
            Bus_Type = "avalon";
            Is_Asynchronous = "0";
            DBS_Big_Endian = "0";
            Adapts_To = "";
            Do_Stream_Reads = "0";
            Do_Stream_Writes = "0";
            Max_Address_Width = "32";
            Data_Width = "32";
            Address_Width = "17";
            Maximum_Burst_Size = "1";
            Register_Incoming_Signals = "0";
            Register_Outgoing_Signals = "0";
            Interleave_Bursts = "0";
            Linewrap_Bursts = "0";
            Burst_On_Burst_Boundaries_Only = "0";
            Always_Burst_Max_Burst = "0";
            Is_Big_Endian = "0";
            Is_Enabled = "1";
            Is_Data_Master = "1";
         }
         PORT_WIRING 
         {
            PORT d_irq
            {
               type = "irq";
               width = "32";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT d_address
            {
               type = "address";
               width = "17";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT d_byteenable
            {
               type = "byteenable";
               width = "4";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT d_read
            {
               type = "read";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT d_readdata
            {
               type = "readdata";
               width = "32";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT d_readdatavalid
            {
               type = "readdatavalid";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT d_waitrequest
            {
               type = "waitrequest";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT d_write
            {
               type = "write";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT d_writedata
            {
               type = "writedata";
               width = "32";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT jtag_debug_module_debugaccess_to_roms
            {
               type = "debugaccess";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
         }
         MEMORY_MAP 
         {
            Entry cpu/jtag_debug_module
            {
               address = "0x00010800";
               span = "0x00000800";
               is_bridge = "0";
            }
            Entry jtag_uart/avalon_jtag_slave
            {
               address = "0x00011010";
               span = "0x00000008";
               is_bridge = "0";
            }
            Entry onchip_memory2/s1
            {
               address = "0x00008000";
               span = "0x00006590";
               is_bridge = "0";
            }
            Entry pio_led/s1
            {
               address = "0x00011000";
               span = "0x00000010";
               is_bridge = "0";
            }
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         cache_has_dcache = "1";
         cache_dcache_size = "2048";
         cache_dcache_line_size = "32";
         cache_dcache_bursts = "0";
         cache_dcache_ram_block_type = "AUTO";
         num_tightly_coupled_data_masters = "0";
         gui_num_tightly_coupled_data_masters = "0";
         gui_include_tightly_coupled_data_masters = "0";
         gui_omit_avalon_data_master = "0";
         cache_has_icache = "1";
         cache_icache_size = "4096";
         cache_icache_line_size = "32";
         cache_icache_ram_block_type = "AUTO";
         cache_icache_bursts = "0";
         num_tightly_coupled_instruction_masters = "0";
         gui_num_tightly_coupled_instruction_masters = "0";
         gui_include_tightly_coupled_instruction_masters = "0";
         debug_level = "2";
         include_oci = "1";
         oci_num_xbrk = "0";
         oci_num_dbrk = "0";
         oci_dbrk_trace = "0";
         oci_dbrk_pairs = "0";
         oci_onchip_trace = "0";
         oci_offchip_trace = "0";
         oci_data_trace = "0";
         include_third_party_debug_port = "0";
         oci_trace_addr_width = "7";
         oci_debugreq_signals = "0";
         oci_trigger_arming = "1";
         oci_embedded_pll = "0";
         oci_assign_jtag_instance_id = "0";
         oci_jtag_instance_id = "0";
         oci_num_pm = "0";
         oci_pm_width = "32";
         performance_counters_present = "0";
         performance_counters_width = "32";
         always_encrypt = "1";
         debug_simgen = "0";
         activate_model_checker = "0";
         activate_test_end_checker = "0";
         activate_trace = "1";
         activate_monitors = "1";
         clear_x_bits_ld_non_bypass = "1";
         bit_31_bypass_dcache = "1";
         hdl_sim_caches_cleared = "1";
         hbreak_test = "0";
         allow_full_address_range = "0";
         extra_exc_info = "0";
         branch_prediction_type = "Dynamic";
         bht_ptr_sz = "8";
         bht_index_pc_only = "0";
         gui_branch_prediction_type = "Automatic";
         full_waveform_signals = "0";
         export_pcb = "0";
         big_endian = "0";
         avalon_debug_port_present = "0";
         illegal_instructions_trap = "0";
         illegal_memory_access_detection = "0";
         illegal_mem_exc = "0";
         slave_access_error_exc = "0";
         division_error_exc = "0";
         eic_present = "0";
         num_shadow_reg_sets = "0";
         gui_mmu_present = "0";
         mmu_present = "0";
         process_id_num_bits = "8";
         tlb_ptr_sz = "7";
         tlb_num_ways = "16";
         udtlb_num_entries = "6";
         uitlb_num_entries = "4";
         fast_tlb_miss_exc_slave = "";
         fast_tlb_miss_exc_offset = "0x00000000";
         mpu_present = "0";
         mpu_num_data_regions = "8";
         mpu_num_inst_regions = "8";
         mpu_min_data_region_size_log2 = "12";
         mpu_min_inst_region_size_log2 = "12";
         mpu_use_limit = "0";
         hardware_divide_present = "0";
         gui_hardware_divide_setting = "0";
         hardware_multiply_present = "1";
         hardware_multiply_impl = "embedded_mul";
         shift_rot_impl = "fast_le_shift";
         gui_hardware_multiply_setting = "embedded_mul_fast_le_shift";
         reset_slave = "onchip_memory2/s1";
         break_slave = "cpu/jtag_debug_module";
         exc_slave = "onchip_memory2/s1";
         reset_offset = "0x00000000";
         break_offset = "0x00000020";
         exc_offset = "0x00000020";
         cpu_reset = "0";
         CPU_Implementation = "fast";
         cpu_selection = "f";
         device_family_id = "CYCLONEIVE";
         address_stall_present = "1";
         dsp_block_supports_shift = "0";
         mrams_present = "0";
         cpuid_value = "0";
         dont_overwrite_cpuid = "1";
         allow_legacy_sdk = "1";
         legacy_sdk_support = "1";
         inst_addr_width = "17";
         data_addr_width = "17";
      }
      class = "altera_nios2";
      class_version = "10.1";
      SYSTEM_BUILDER_INFO 
      {
         Is_Enabled = "1";
         Clock_Source = "clk_50";
         Has_Clock = "1";
      }
   }
   MODULE jtag_uart
   {
      SLAVE avalon_jtag_slave
      {
         PORT_WIRING 
         {
            PORT clk
            {
               type = "clk";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT rst_n
            {
               type = "reset_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT av_irq
            {
               type = "irq";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT av_chipselect
            {
               type = "chipselect";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT av_address
            {
               type = "address";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT av_read_n
            {
               type = "read_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT av_readdata
            {
               type = "readdata";
               width = "32";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT av_write_n
            {
               type = "write_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT av_writedata
            {
               type = "writedata";
               width = "32";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT av_waitrequest
            {
               type = "waitrequest";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT dataavailable
            {
               type = "dataavailable";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT readyfordata
            {
               type = "readyfordata";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Has_IRQ = "1";
            Bus_Type = "avalon";
            Read_Wait_States = "peripheral_controlled";
            Write_Wait_States = "peripheral_controlled";
            Hold_Time = "0cycles";
            Setup_Time = "0cycles";
            Is_Printable_Device = "1";
            Address_Alignment = "native";
            Well_Behaved_Waitrequest = "0";
            Is_Nonvolatile_Storage = "0";
            Read_Latency = "0";
            Is_Memory_Device = "0";
            Maximum_Pending_Read_Transactions = "0";
            Minimum_Uninterrupted_Run_Length = "1";
            Accepts_Internal_Connections = "1";
            Write_Latency = "0";
            Is_Flash = "0";
            Data_Width = "32";
            Address_Width = "1";
            Maximum_Burst_Size = "1";
            Register_Incoming_Signals = "0";
            Register_Outgoing_Signals = "0";
            Interleave_Bursts = "0";
            Linewrap_Bursts = "0";
            Burst_On_Burst_Boundaries_Only = "0";
            Always_Burst_Max_Burst = "0";
            Is_Big_Endian = "0";
            Is_Enabled = "1";
            JTAG_Hub_Base_Id = "262254";
            JTAG_Hub_Instance_Id = "0";
            Connection_Limit = "1";
            MASTERED_BY cpu/data_master
            {
               priority = "1";
               Offset_Address = "0x00011010";
            }
            IRQ_MASTER cpu/data_master
            {
               IRQ_Number = "0";
            }
            Base_Address = "0x00011010";
         }
      }
      class = "altera_avalon_jtag_uart";
      class_version = "10.1";
      iss_model_name = "altera_avalon_jtag_uart";
      WIZARD_SCRIPT_ARGUMENTS 
      {
         write_depth = "64";
         read_depth = "64";
         write_threshold = "8";
         read_threshold = "8";
         read_char_stream = "";
         showascii = "1";
         relativepath = "1";
         read_le = "0";
         write_le = "0";
         altera_show_unreleased_jtag_uart_features = "0";
      }
      SIMULATION 
      {
         DISPLAY 
         {
            SIGNAL av_chipselect
            {
               name = "av_chipselect";
            }
            SIGNAL av_address
            {
               name = "av_address";
            }
            SIGNAL av_read_n
            {
               name = "av_read_n";
            }
            SIGNAL av_readdata
            {
               name = "av_readdata";
               radix = "hexadecimal";
            }
            SIGNAL av_write_n
            {
               name = "av_write_n";
            }
            SIGNAL av_writedata
            {
               name = "av_writedata";
               radix = "hexadecimal";
            }
            SIGNAL av_waitrequest
            {
               name = "av_waitrequest";
            }
            SIGNAL dataavailable
            {
               name = "dataavailable";
            }
            SIGNAL readyfordata
            {
               name = "readyfordata";
            }
         }
         INTERACTIVE_IN drive
         {
            enable = "0";
            file = "_input_data_stream.dat";
            mutex = "_input_data_mutex.dat";
            log = "_in.log";
            rate = "100";
            signals = "temp,list";
            exe = "nios2-terminal";
         }
         INTERACTIVE_OUT log
         {
            enable = "1";
            exe = "perl -- atail-f.pl";
            file = "_output_stream.dat";
            radix = "ascii";
            signals = "temp,list";
         }
      }
      SYSTEM_BUILDER_INFO 
      {
         Is_Enabled = "1";
         Clock_Source = "clk_50";
         Has_Clock = "1";
      }
   }
   MODULE onchip_memory2
   {
      SLAVE s1
      {
         PORT_WIRING 
         {
            PORT clk
            {
               type = "clk";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT reset
            {
               type = "reset";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT address
            {
               type = "address";
               width = "13";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT chipselect
            {
               type = "chipselect";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT clken
            {
               type = "clken";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT readdata
            {
               type = "readdata";
               width = "32";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT write
            {
               type = "write";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT writedata
            {
               type = "writedata";
               width = "32";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT byteenable
            {
               type = "byteenable";
               width = "4";
               direction = "input";
               Is_Enabled = "1";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Write_Wait_States = "0cycles";
            Read_Wait_States = "0cycles";
            Hold_Time = "0cycles";
            Setup_Time = "0cycles";
            Is_Printable_Device = "0";
            Address_Alignment = "dynamic";
            Well_Behaved_Waitrequest = "0";
            Is_Nonvolatile_Storage = "0";
            Address_Span = "26000";
            Read_Latency = "1";
            Is_Memory_Device = "1";
            Maximum_Pending_Read_Transactions = "0";
            Minimum_Uninterrupted_Run_Length = "1";
            Accepts_Internal_Connections = "1";
            Write_Latency = "0";
            Is_Flash = "0";
            Data_Width = "32";
            Address_Width = "13";
            Maximum_Burst_Size = "1";
            Register_Incoming_Signals = "0";
            Register_Outgoing_Signals = "0";
            Interleave_Bursts = "0";
            Linewrap_Bursts = "0";
            Burst_On_Burst_Boundaries_Only = "0";
            Always_Burst_Max_Burst = "0";
            Is_Big_Endian = "0";
            Is_Enabled = "1";
            MASTERED_BY cpu/instruction_master
            {
               priority = "1";
               Offset_Address = "0x00008000";
            }
            MASTERED_BY cpu/data_master
            {
               priority = "1";
               Offset_Address = "0x00008000";
            }
            Base_Address = "0x00008000";
         }
      }
      iss_model_name = "altera_memory";
      WIZARD_SCRIPT_ARGUMENTS 
      {
         allow_mram_sim_contents_only_file = "0";
         ram_block_type = "AUTO";
         init_contents_file = "onchip_memory2";
         non_default_init_file_enabled = "0";
         gui_ram_block_type = "Automatic";
         Writeable = "1";
         dual_port = "0";
         Size_Value = "26000";
         Size_Multiple = "1";
         use_shallow_mem_blocks = "0";
         init_mem_content = "1";
         allow_in_system_memory_content_editor = "0";
         instance_id = "NONE";
         read_during_write_mode = "DONT_CARE";
         ignore_auto_block_type_assignment = "1";
      }
      SIMULATION 
      {
         DISPLAY 
         {
            SIGNAL a
            {
               name = "chipselect";
               conditional = "1";
            }
            SIGNAL c
            {
               name = "address";
               radix = "hexadecimal";
            }
            SIGNAL d
            {
               name = "byteenable";
               radix = "binary";
               conditional = "1";
            }
            SIGNAL e
            {
               name = "readdata";
               radix = "hexadecimal";
            }
            SIGNAL b
            {
               name = "write";
               conditional = "1";
            }
            SIGNAL f
            {
               name = "writedata";
               radix = "hexadecimal";
               conditional = "1";
            }
         }
      }
      SYSTEM_BUILDER_INFO 
      {
         Prohibited_Device_Family = "MERCURY, APEX20K, APEX20KE, APEX20KC, APEXII, ACEX1K, FLEX10KE, EXCALIBUR_ARM, MAXII";
         Instantiate_In_System_Module = "1";
         Is_Enabled = "1";
         Default_Module_Name = "onchip_memory";
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk_50";
         Has_Clock = "1";
      }
      class = "altera_avalon_onchip_memory2";
      class_version = "10.1";
   }
   MODULE pio_led
   {
      SLAVE s1
      {
         PORT_WIRING 
         {
            PORT clk
            {
               type = "clk";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT reset_n
            {
               type = "reset_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT address
            {
               type = "address";
               width = "2";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT write_n
            {
               type = "write_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT writedata
            {
               type = "writedata";
               width = "8";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT chipselect
            {
               type = "chipselect";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT readdata
            {
               type = "readdata";
               width = "8";
               direction = "output";
               Is_Enabled = "1";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Write_Wait_States = "0cycles";
            Read_Wait_States = "1cycles";
            Hold_Time = "0cycles";
            Setup_Time = "0cycles";
            Is_Printable_Device = "0";
            Address_Alignment = "native";
            Well_Behaved_Waitrequest = "0";
            Is_Nonvolatile_Storage = "0";
            Read_Latency = "0";
            Is_Memory_Device = "0";
            Maximum_Pending_Read_Transactions = "0";
            Minimum_Uninterrupted_Run_Length = "1";
            Accepts_Internal_Connections = "1";
            Write_Latency = "0";
            Is_Flash = "0";
            Data_Width = "8";
            Address_Width = "2";
            Maximum_Burst_Size = "1";
            Register_Incoming_Signals = "0";
            Register_Outgoing_Signals = "0";
            Interleave_Bursts = "0";
            Linewrap_Bursts = "0";
            Burst_On_Burst_Boundaries_Only = "0";
            Always_Burst_Max_Burst = "0";
            Is_Big_Endian = "0";
            Is_Enabled = "1";
            MASTERED_BY cpu/data_master
            {
               priority = "1";
               Offset_Address = "0x00011000";
            }
            Base_Address = "0x00011000";
         }
      }
      PORT_WIRING 
      {
         PORT out_port
         {
            type = "export";
            width = "8";
            direction = "output";
            Is_Enabled = "1";
         }
      }
      class = "altera_avalon_pio";
      class_version = "10.1";
      SYSTEM_BUILDER_INFO 
      {
         Is_Enabled = "1";
         Instantiate_In_System_Module = "1";
         Wire_Test_Bench_Values = "1";
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk_50";
         Has_Clock = "1";
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         Do_Test_Bench_Wiring = "0";
         Driven_Sim_Value = "0";
         has_tri = "0";
         has_out = "1";
         has_in = "0";
         capture = "0";
         Data_Width = "8";
         reset_value = "0";
         edge_type = "NONE";
         irq_type = "NONE";
         bit_clearing_edge_register = "0";
         bit_modifying_output_register = "0";
      }
   }
}
