SYSTEM DE0_NANO_SOPC
{
   System_Wizard_Version = "10.10";
   System_Wizard_Build = "153";
   Builder_Application = "sopc_builder_ca";
   WIZARD_SCRIPT_ARGUMENTS 
   {
      hdl_language = "verilog";
      device_family = "CYCLONEIVE";
      device_family_id = "CYCLONEIVE";
      generate_sdk = "0";
      do_build_sim = "0";
      hardcopy_compatible = "0";
      CLOCKS 
      {
         CLOCK clk_50
         {
            frequency = "50000000";
            source = "External";
            Is_Clock_Source = "0";
            display_name = "clk_50";
            pipeline = "0";
            clock_module_connection_point_for_c2h = "clk_50.clk";
         }
      }
      clock_freq = "50000000";
      clock_freq = "50000000";
      board_class = "";
      view_master_columns = "1";
      view_master_priorities = "0";
      generate_hdl = "";
      bustype_column_width = "0";
      clock_column_width = "80";
      name_column_width = "75";
      desc_column_width = "75";
      base_column_width = "75";
      end_column_width = "75";
      do_log_history = "0";
   }
   MODULE cpu
   {
      MASTER instruction_master
      {
         PORT_WIRING 
         {
            PORT clk
            {
               type = "clk";
               width = "1";
               direction = "input";
               Is_Enabled = "0";
            }
            PORT reset_n
            {
               type = "reset_n";
               width = "1";
               direction = "input";
               Is_Enabled = "0";
            }
            PORT i_address
            {
               type = "address";
               width = "17";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT i_read
            {
               type = "read";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT i_readdata
            {
               type = "readdata";
               width = "32";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT i_readdatavalid
            {
               type = "readdatavalid";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT i_waitrequest
            {
               type = "waitrequest";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT jtag_debug_module_resetrequest
            {
               type = "resetrequest";
               width = "1";
               direction = "output";
               Is_Enabled = "0";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Is_Asynchronous = "0";
            DBS_Big_Endian = "0";
            Adapts_To = "";
            Do_Stream_Reads = "0";
            Do_Stream_Writes = "0";
            Max_Address_Width = "32";
            Data_Width = "32";
            Address_Width = "17";
            Maximum_Burst_Size = "1";
            Register_Incoming_Signals = "0";
            Register_Outgoing_Signals = "0";
            Interleave_Bursts = "";
            Linewrap_Bursts = "";
            Burst_On_Burst_Boundaries_Only = "";
            Always_Burst_Max_Burst = "";
            Is_Big_Endian = "0";
            Is_Enabled = "1";
            Is_Instruction_Master = "1";
            Is_Readable = "1";
            Is_Writeable = "0";
            Address_Group = "0";
            Has_IRQ = "0";
            Irq_Scheme = "individual_requests";
            Interrupt_Range = "0-0";
         }
         MEMORY_MAP 
         {
            Entry cpu/jtag_debug_module
            {
               address = "0x00010800";
               span = "0x00000800";
               is_bridge = "0";
            }
            Entry onchip_memory2/s1
            {
               address = "0x00008000";
               span = "0x00006590";
               is_bridge = "0";
            }
         }
      }
      MASTER custom_instruction_master
      {
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "nios_custom_instruction";
            Data_Width = "32";
            Address_Width = "8";
            Is_Custom_Instruction = "1";
            Is_Enabled = "0";
            Max_Address_Width = "8";
            Base_Address = "N/A";
            Is_Visible = "0";
         }
         PORT_WIRING 
         {
            PORT dataa
            {
               type = "dataa";
               width = "32";
               direction = "output";
            }
            PORT datab
            {
               type = "datab";
               width = "32";
               direction = "output";
            }
            PORT result
            {
               type = "result";
               width = "32";
               direction = "input";
            }
            PORT clk_en
            {
               type = "clk_en";
               width = "1";
               direction = "output";
            }
            PORT reset
            {
               type = "reset";
               width = "1";
               direction = "output";
            }
            PORT start
            {
               type = "start";
               width = "1";
               direction = "output";
            }
            PORT done
            {
               type = "done";
               width = "1";
               direction = "input";
            }
            PORT n
            {
               type = "n";
               width = "8";
               direction = "output";
            }
            PORT a
            {
               type = "a";
               width = "5";
               direction = "output";
            }
            PORT b
            {
               type = "b";
               width = "5";
               direction = "output";
            }
            PORT c
            {
               type = "c";
               width = "5";
               direction = "output";
            }
            PORT readra
            {
               type = "readra";
               width = "1";
               direction = "output";
            }
            PORT readrb
            {
               type = "readrb";
               width = "1";
               direction = "output";
            }
            PORT writerc
            {
               type = "writerc";
               width = "1";
               direction = "output";
            }
         }
      }
      SLAVE jtag_debug_module
      {
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Write_Wait_States = "0cycles";
            Read_Wait_States = "1cycles";
            Hold_Time = "0cycles";
            Setup_Time = "0cycles";
            Is_Printable_Device = "0";
            Address_Alignment = "dynamic";
            Well_Behaved_Waitrequest = "0";
            Is_Nonvolatile_Storage = "0";
            Address_Span = "2048";
            Read_Latency = "0";
            Is_Memory_Device = "1";
            Maximum_Pending_Read_Transactions = "0";
            Minimum_Uninterrupted_Run_Length = "1";
            Accepts_Internal_Connections = "1";
            Write_Latency = "0";
            Is_Flash = "0";
            Data_Width = "32";
            Address_Width = "9";
            Maximum_Burst_Size = "1";
            Register_Incoming_Signals = "0";
            Register_Outgoing_Signals = "0";
            Interleave_Bursts = "0";
            Linewrap_Bursts = "0";
            Burst_On_Burst_Boundaries_Only = "0";
            Always_Burst_Max_Burst = "0";
            Is_Big_Endian = "0";
            Is_Enabled = "1";
            Accepts_External_Connections = "1";
            Requires_Internal_Connections = "";
            MASTERED_BY cpu/instruction_master
            {
               priority = "1";
               Offset_Address = "0x00010800";
            }
            MASTERED_BY cpu/data_master
            {
               priority = "1";
               Offset_Address = "0x00010800";
            }
            Base_Address = "0x00010800";
            Is_Readable = "1";
            Is_Writeable = "1";
            Uses_Tri_State_Data_Bus = "0";
            Has_IRQ = "0";
            JTAG_Hub_Base_Id = "1118278";
            JTAG_Hub_Instance_Id = "0";
            Address_Group = "0";
            IRQ_MASTER cpu/data_master
            {
               IRQ_Number = "NC";
            }
         }
         PORT_WIRING 
         {
            PORT jtag_debug_module_address
            {
               type = "address";
               width = "9";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT jtag_debug_module_begintransfer
            {
               type = "begintransfer";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT jtag_debug_module_byteenable
            {
               type = "byteenable";
               width = "4";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT jtag_debug_module_debugaccess
            {
               type = "debugaccess";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT jtag_debug_module_readdata
            {
               type = "readdata";
               width = "32";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT jtag_debug_module_select
            {
               type = "chipselect";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT jtag_debug_module_write
            {
               type = "write";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT jtag_debug_module_writedata
            {
               type = "writedata";
               width = "32";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT clk
            {
               Is_Enabled = "1";
               direction = "input";
               type = "clk";
               width = "1";
            }
            PORT jtag_debug_module_resetrequest
            {
               Is_Enabled = "1";
               direction = "output";
               type = "resetrequest";
               width = "1";
            }
            PORT reset_n
            {
               Is_Enabled = "1";
               direction = "input";
               type = "reset_n";
               width = "1";
            }
         }
      }
      MASTER data_master
      {
         SYSTEM_BUILDER_INFO 
         {
            Has_IRQ = "1";
            Irq_Scheme = "individual_requests";
            Bus_Type = "avalon";
            Is_Asynchronous = "0";
            DBS_Big_Endian = "0";
            Adapts_To = "";
            Do_Stream_Reads = "0";
            Do_Stream_Writes = "0";
            Max_Address_Width = "32";
            Data_Width = "32";
            Address_Width = "17";
            Maximum_Burst_Size = "1";
            Register_Incoming_Signals = "0";
            Register_Outgoing_Signals = "0";
            Interleave_Bursts = "0";
            Linewrap_Bursts = "0";
            Burst_On_Burst_Boundaries_Only = "";
            Always_Burst_Max_Burst = "0";
            Is_Big_Endian = "0";
            Is_Enabled = "1";
            Is_Data_Master = "1";
            Address_Group = "0";
            Is_Readable = "1";
            Is_Writeable = "1";
            Interrupt_Range = "0-31";
         }
         PORT_WIRING 
         {
            PORT d_irq
            {
               type = "irq";
               width = "32";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT d_address
            {
               type = "address";
               width = "17";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT d_byteenable
            {
               type = "byteenable";
               width = "4";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT d_read
            {
               type = "read";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT d_readdata
            {
               type = "readdata";
               width = "32";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT d_readdatavalid
            {
               type = "readdatavalid";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT d_waitrequest
            {
               type = "waitrequest";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT d_write
            {
               type = "write";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT d_writedata
            {
               type = "writedata";
               width = "32";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT jtag_debug_module_debugaccess_to_roms
            {
               type = "debugaccess";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
         }
         MEMORY_MAP 
         {
            Entry cpu/jtag_debug_module
            {
               address = "0x00010800";
               span = "0x00000800";
               is_bridge = "0";
            }
            Entry jtag_uart/avalon_jtag_slave
            {
               address = "0x00011010";
               span = "0x00000008";
               is_bridge = "0";
            }
            Entry onchip_memory2/s1
            {
               address = "0x00008000";
               span = "0x00006590";
               is_bridge = "0";
            }
            Entry pio_led/s1
            {
               address = "0x00011000";
               span = "0x00000010";
               is_bridge = "0";
            }
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         cache_has_dcache = "1";
         cache_dcache_size = "2048";
         cache_dcache_line_size = "32";
         cache_dcache_bursts = "0";
         cache_dcache_ram_block_type = "AUTO";
         num_tightly_coupled_data_masters = "0";
         gui_num_tightly_coupled_data_masters = "0";
         gui_include_tightly_coupled_data_masters = "0";
         gui_omit_avalon_data_master = "0";
         cache_has_icache = "1";
         cache_icache_size = "4096";
         cache_icache_line_size = "32";
         cache_icache_ram_block_type = "AUTO";
         cache_icache_bursts = "0";
         num_tightly_coupled_instruction_masters = "0";
         gui_num_tightly_coupled_instruction_masters = "0";
         gui_include_tightly_coupled_instruction_masters = "0";
         debug_level = "2";
         include_oci = "1";
         oci_num_xbrk = "0";
         oci_num_dbrk = "0";
         oci_dbrk_trace = "0";
         oci_dbrk_pairs = "0";
         oci_onchip_trace = "0";
         oci_offchip_trace = "0";
         oci_data_trace = "0";
         include_third_party_debug_port = "0";
         oci_trace_addr_width = "7";
         oci_debugreq_signals = "0";
         oci_trigger_arming = "1";
         oci_embedded_pll = "0";
         oci_assign_jtag_instance_id = "0";
         oci_jtag_instance_id = "0";
         oci_num_pm = "0";
         oci_pm_width = "32";
         performance_counters_present = "0";
         performance_counters_width = "32";
         always_encrypt = "1";
         debug_simgen = "0";
         activate_model_checker = "0";
         activate_test_end_checker = "0";
         activate_trace = "1";
         activate_monitors = "1";
         clear_x_bits_ld_non_bypass = "1";
         bit_31_bypass_dcache = "1";
         hdl_sim_caches_cleared = "1";
         hbreak_test = "0";
         allow_full_address_range = "0";
         extra_exc_info = "0";
         branch_prediction_type = "Dynamic";
         bht_ptr_sz = "8";
         bht_index_pc_only = "0";
         gui_branch_prediction_type = "Automatic";
         full_waveform_signals = "0";
         export_pcb = "0";
         big_endian = "0";
         avalon_debug_port_present = "0";
         illegal_instructions_trap = "0";
         illegal_memory_access_detection = "0";
         illegal_mem_exc = "0";
         slave_access_error_exc = "0";
         division_error_exc = "0";
         eic_present = "0";
         num_shadow_reg_sets = "0";
         gui_mmu_present = "0";
         mmu_present = "0";
         process_id_num_bits = "8";
         tlb_ptr_sz = "7";
         tlb_num_ways = "16";
         udtlb_num_entries = "6";
         uitlb_num_entries = "4";
         fast_tlb_miss_exc_slave = "";
         fast_tlb_miss_exc_offset = "0x00000000";
         mpu_present = "0";
         mpu_num_data_regions = "8";
         mpu_num_inst_regions = "8";
         mpu_min_data_region_size_log2 = "12";
         mpu_min_inst_region_size_log2 = "12";
         mpu_use_limit = "0";
         hardware_divide_present = "0";
         gui_hardware_divide_setting = "0";
         hardware_multiply_present = "1";
         hardware_multiply_impl = "embedded_mul";
         shift_rot_impl = "fast_le_shift";
         gui_hardware_multiply_setting = "embedded_mul_fast_le_shift";
         reset_slave = "onchip_memory2/s1";
         break_slave = "cpu/jtag_debug_module";
         exc_slave = "onchip_memory2/s1";
         reset_offset = "0x00000000";
         break_offset = "0x00000020";
         exc_offset = "0x00000020";
         cpu_reset = "0";
         CPU_Implementation = "fast";
         cpu_selection = "f";
         device_family_id = "CYCLONEIVE";
         address_stall_present = "1";
         dsp_block_supports_shift = "0";
         mrams_present = "0";
         cpuid_value = "0";
         dont_overwrite_cpuid = "1";
         allow_legacy_sdk = "1";
         legacy_sdk_support = "1";
         inst_addr_width = "17";
         data_addr_width = "17";
         CPU_Architecture = "nios2";
         cache_icache_burst_type = "none";
         oci_sync_depth = "2";
         hardware_divide_impl = "variable_latency";
         hardware_multiply_omits_msw = "1";
         break_slave_override = "";
         break_offset_override = "0x20";
         altera_show_unreleased_features = "0";
         altera_show_unpublished_features = "0";
         altera_internal_test = "0";
         alt_log_port_base = "";
         alt_log_port_type = "";
         cpuid_sz = "1";
         gui_illegal_instructions_trap = "0";
         advanced_exc = "0";
         gui_illegal_memory_access_detection = "0";
         cache_omit_dcache = "0";
         cache_omit_icache = "0";
         omit_instruction_master = "0";
         omit_data_master = "0";
         ras_ptr_sz = "4";
         jtb_ptr_sz = "5";
         ibuf_ptr_sz = "4";
         always_bypass_dcache = "0";
         iss_trace_on = "0";
         iss_trace_warning = "1";
         iss_trace_info = "1";
         iss_trace_disassembly = "0";
         iss_trace_registers = "0";
         iss_trace_instr_count = "0";
         iss_software_debug = "0";
         iss_software_debug_port = "9996";
         iss_memory_dump_start = "";
         iss_memory_dump_end = "";
         Boot_Copier = "boot_loader_cfi.srec";
         Boot_Copier_EPCS = "boot_loader_epcs.srec";
         Boot_Copier_EPCS_SII_SIII_CIII = "boot_loader_epcs_sii_siii_ciii.srec";
         Boot_Copier_BE = "boot_loader_cfi_be.srec";
         Boot_Copier_EPCS_BE = "boot_loader_epcs_be.srec";
         Boot_Copier_EPCS_SII_SIII_CIII_BE = "boot_loader_epcs_sii_siii_ciii_be.srec";
         CONSTANTS 
         {
            CONSTANT __nios_catch_irqs__
            {
               value = "1";
               comment = "Include panic handler for all irqs (needs uart)";
            }
            CONSTANT __nios_use_constructors__
            {
               value = "1";
               comment = "Call c++ static constructors";
            }
            CONSTANT __nios_use_small_printf__
            {
               value = "1";
               comment = "Smaller non-ANSI printf, with no floating point";
            }
            CONSTANT nasys_has_icache
            {
               value = "1";
               comment = "True if instruction cache present";
            }
            CONSTANT nasys_icache_size
            {
               value = "4096";
               comment = "Size in bytes of instruction cache";
            }
            CONSTANT nasys_icache_line_size
            {
               value = "32";
               comment = "Size in bytes of each icache line";
            }
            CONSTANT nasys_icache_line_size_log2
            {
               value = "5";
               comment = "Log2 size in bytes of each icache line";
            }
            CONSTANT nasys_has_dcache
            {
               value = "1";
               comment = "True if instruction cache present";
            }
            CONSTANT nasys_dcache_size
            {
               value = "2048";
               comment = "Size in bytes of data cache";
            }
            CONSTANT nasys_dcache_line_size
            {
               value = "32";
               comment = "Size in bytes of each dcache line";
            }
            CONSTANT nasys_dcache_line_size_log2
            {
               value = "5";
               comment = "Log2 size in bytes of each dcache line";
            }
         }
         license_status = "encrypted";
         mainmem_slave = "onchip_memory2/s1";
         datamem_slave = "onchip_memory2/s1";
         maincomm_slave = "";
         germs_monitor_id = "";
      }
      class = "altera_nios2";
      class_version = "7.08101";
      SYSTEM_BUILDER_INFO 
      {
         Is_Enabled = "1";
         Clock_Source = "clk_50";
         Has_Clock = "1";
         Parameters_Signature = "";
         Is_CPU = "1";
         Instantiate_In_System_Module = "1";
         Required_Device_Family = "STRATIX,STRATIXGX,STRATIXII,STRATIXIIGX,STRATIXIIGXLITE,STRATIXIII,STRATIXIV,STRATIXV,CYCLONE,CYCLONEII,CYCLONEIII,CYCLONEIVE,HARDCOPYIII,ARRIAII,ARRIAIIGZ,TARPON,HARDCOPYIV,STINGRAY";
         Default_Module_Name = "cpu";
         Top_Level_Ports_Are_Enumerated = "1";
         View 
         {
            Settings_Summary = "Nios II/f
            <br>&nbsp;&nbsp;4-Kbyte Instruction Cache
            <br>&nbsp;&nbsp;2-Kbyte Data Cache
            <br>&nbsp;&nbsp;JTAG Debug Module
            ";
            MESSAGES 
            {
            }
         }
      }
      iss_model_name = "altera_nios2";
      HDL_INFO 
      {
         PLI_Files = "";
         Precompiled_Simulation_Library_Files = "";
         Simulation_HDL_Files = "";
         Synthesis_HDL_Files = "__PROJECT_DIRECTORY__/cpu_test_bench.v, __PROJECT_DIRECTORY__/cpu_mult_cell.v, __PROJECT_DIRECTORY__/cpu_oci_test_bench.v, __PROJECT_DIRECTORY__/cpu_jtag_debug_module_tck.v, __PROJECT_DIRECTORY__/cpu_jtag_debug_module_sysclk.v, __PROJECT_DIRECTORY__/cpu_jtag_debug_module_wrapper.v, __PROJECT_DIRECTORY__/cpu.v";
         Synthesis_Only_Files = "";
      }
      MASTER tightly_coupled_instruction_master_0
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "0";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Is_Instruction_Master = "1";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Is_Big_Endian = "0";
            Connection_Limit = "1";
            Is_Channel = "1";
         }
      }
      MASTER tightly_coupled_instruction_master_1
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "0";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Address_Group = "0";
            Is_Instruction_Master = "1";
            Is_Readable = "1";
            Is_Writeable = "0";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Is_Big_Endian = "0";
            Connection_Limit = "1";
            Is_Channel = "1";
         }
      }
      MASTER tightly_coupled_instruction_master_2
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "0";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Address_Group = "0";
            Is_Instruction_Master = "1";
            Is_Readable = "1";
            Is_Writeable = "0";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Is_Big_Endian = "0";
            Connection_Limit = "1";
            Is_Channel = "1";
         }
      }
      MASTER tightly_coupled_instruction_master_3
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "0";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Address_Group = "0";
            Is_Instruction_Master = "1";
            Is_Readable = "1";
            Is_Writeable = "0";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Is_Big_Endian = "0";
            Connection_Limit = "1";
            Is_Channel = "1";
         }
      }
      MASTER data_master2
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "1";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Address_Group = "0";
            Is_Data_Master = "1";
            Is_Readable = "1";
            Is_Writeable = "1";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Is_Big_Endian = "0";
         }
      }
      MASTER tightly_coupled_data_master_0
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "0";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Address_Group = "0";
            Is_Data_Master = "1";
            Is_Readable = "1";
            Is_Writeable = "1";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Is_Big_Endian = "0";
            Connection_Limit = "1";
            Is_Channel = "1";
         }
      }
      MASTER tightly_coupled_data_master_1
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "0";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Address_Group = "0";
            Is_Data_Master = "1";
            Is_Readable = "1";
            Is_Writeable = "1";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Is_Big_Endian = "0";
            Connection_Limit = "1";
            Is_Channel = "1";
         }
      }
      MASTER tightly_coupled_data_master_2
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "0";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Address_Group = "0";
            Is_Data_Master = "1";
            Is_Readable = "1";
            Is_Writeable = "1";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Is_Big_Endian = "0";
            Connection_Limit = "1";
            Is_Channel = "1";
         }
      }
      MASTER tightly_coupled_data_master_3
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "0";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Address_Group = "0";
            Is_Data_Master = "1";
            Is_Readable = "1";
            Is_Writeable = "1";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Is_Big_Endian = "0";
            Connection_Limit = "1";
            Is_Channel = "1";
         }
      }
      PORT_WIRING 
      {
         PORT jtag_debug_trigout
         {
            width = "1";
            direction = "output";
            Is_Enabled = "0";
         }
         PORT jtag_debug_offchip_trace_clk
         {
            width = "1";
            direction = "output";
            Is_Enabled = "0";
         }
         PORT jtag_debug_offchip_trace_data
         {
            width = "18";
            direction = "output";
            Is_Enabled = "0";
         }
         PORT clkx2
         {
            width = "1";
            direction = "input";
            Is_Enabled = "0";
            visible = "0";
         }
      }
      SIMULATION 
      {
         DISPLAY 
         {
            SIGNAL aaa
            {
               format = "Logic";
               name = "i_readdata";
               radix = "hexadecimal";
            }
            SIGNAL aab
            {
               format = "Logic";
               name = "i_readdatavalid";
               radix = "hexadecimal";
            }
            SIGNAL aac
            {
               format = "Logic";
               name = "i_waitrequest";
               radix = "hexadecimal";
            }
            SIGNAL aad
            {
               format = "Logic";
               name = "i_address";
               radix = "hexadecimal";
            }
            SIGNAL aae
            {
               format = "Logic";
               name = "i_read";
               radix = "hexadecimal";
            }
            SIGNAL aaf
            {
               format = "Logic";
               name = "clk";
               radix = "hexadecimal";
            }
            SIGNAL aag
            {
               format = "Logic";
               name = "reset_n";
               radix = "hexadecimal";
            }
            SIGNAL aah
            {
               format = "Logic";
               name = "d_readdata";
               radix = "hexadecimal";
            }
            SIGNAL aai
            {
               format = "Logic";
               name = "d_waitrequest";
               radix = "hexadecimal";
            }
            SIGNAL aaj
            {
               format = "Logic";
               name = "d_address";
               radix = "hexadecimal";
            }
            SIGNAL aak
            {
               format = "Logic";
               name = "d_byteenable";
               radix = "hexadecimal";
            }
            SIGNAL aal
            {
               format = "Logic";
               name = "d_read";
               radix = "hexadecimal";
            }
            SIGNAL aam
            {
               format = "Logic";
               name = "d_write";
               radix = "hexadecimal";
            }
            SIGNAL aan
            {
               format = "Logic";
               name = "d_writedata";
               radix = "hexadecimal";
            }
            SIGNAL aao
            {
               format = "Logic";
               name = "d_irq";
               radix = "hexadecimal";
            }
            SIGNAL aap
            {
               format = "Logic";
               name = "d_readdatavalid";
               radix = "hexadecimal";
            }
            SIGNAL aaq
            {
               format = "Divider";
               name = "base pipeline";
               radix = "";
            }
            SIGNAL aar
            {
               format = "Logic";
               name = "clk";
               radix = "hexadecimal";
            }
            SIGNAL aas
            {
               format = "Logic";
               name = "reset_n";
               radix = "hexadecimal";
            }
            SIGNAL aat
            {
               format = "Logic";
               name = "D_stall";
               radix = "hexadecimal";
            }
            SIGNAL aau
            {
               format = "Logic";
               name = "A_stall";
               radix = "hexadecimal";
            }
            SIGNAL aav
            {
               format = "Logic";
               name = "F_pcb_nxt";
               radix = "hexadecimal";
            }
            SIGNAL aaw
            {
               format = "Logic";
               name = "F_pcb";
               radix = "hexadecimal";
            }
            SIGNAL aax
            {
               format = "Logic";
               name = "D_pcb";
               radix = "hexadecimal";
            }
            SIGNAL aay
            {
               format = "Logic";
               name = "E_pcb";
               radix = "hexadecimal";
            }
            SIGNAL aaz
            {
               format = "Logic";
               name = "M_pcb";
               radix = "hexadecimal";
            }
            SIGNAL aba
            {
               format = "Logic";
               name = "A_pcb";
               radix = "hexadecimal";
            }
            SIGNAL abb
            {
               format = "Logic";
               name = "W_pcb";
               radix = "hexadecimal";
            }
            SIGNAL abc
            {
               format = "Logic";
               name = "F_vinst";
               radix = "ascii";
            }
            SIGNAL abd
            {
               format = "Logic";
               name = "D_vinst";
               radix = "ascii";
            }
            SIGNAL abe
            {
               format = "Logic";
               name = "E_vinst";
               radix = "ascii";
            }
            SIGNAL abf
            {
               format = "Logic";
               name = "M_vinst";
               radix = "ascii";
            }
            SIGNAL abg
            {
               format = "Logic";
               name = "A_vinst";
               radix = "ascii";
            }
            SIGNAL abh
            {
               format = "Logic";
               name = "W_vinst";
               radix = "ascii";
            }
            SIGNAL abi
            {
               format = "Logic";
               name = "F_inst_ram_hit";
               radix = "hexadecimal";
            }
            SIGNAL abj
            {
               format = "Logic";
               name = "F_iw_valid";
               radix = "hexadecimal";
            }
            SIGNAL abk
            {
               format = "Logic";
               name = "F_issue";
               radix = "hexadecimal";
            }
            SIGNAL abl
            {
               format = "Logic";
               name = "F_kill";
               radix = "hexadecimal";
            }
            SIGNAL abm
            {
               format = "Logic";
               name = "D_kill";
               radix = "hexadecimal";
            }
            SIGNAL abn
            {
               format = "Logic";
               name = "D_refetch";
               radix = "hexadecimal";
            }
            SIGNAL abo
            {
               format = "Logic";
               name = "D_issue";
               radix = "hexadecimal";
            }
            SIGNAL abp
            {
               format = "Logic";
               name = "D_valid";
               radix = "hexadecimal";
            }
            SIGNAL abq
            {
               format = "Logic";
               name = "D_rdprs_stall";
               radix = "hexadecimal";
            }
            SIGNAL abr
            {
               format = "Logic";
               name = "D_rdprs_stall_done";
               radix = "hexadecimal";
            }
            SIGNAL abs
            {
               format = "Logic";
               name = "E_valid";
               radix = "hexadecimal";
            }
            SIGNAL abt
            {
               format = "Logic";
               name = "M_valid";
               radix = "hexadecimal";
            }
            SIGNAL abu
            {
               format = "Logic";
               name = "A_valid";
               radix = "hexadecimal";
            }
            SIGNAL abv
            {
               format = "Logic";
               name = "W_valid";
               radix = "hexadecimal";
            }
            SIGNAL abw
            {
               format = "Logic";
               name = "W_wr_dst_reg";
               radix = "hexadecimal";
            }
            SIGNAL abx
            {
               format = "Logic";
               name = "W_dst_regnum";
               radix = "hexadecimal";
            }
            SIGNAL aby
            {
               format = "Logic";
               name = "W_wr_data";
               radix = "hexadecimal";
            }
            SIGNAL abz
            {
               format = "Logic";
               name = "D_en";
               radix = "hexadecimal";
            }
            SIGNAL aca
            {
               format = "Logic";
               name = "E_en";
               radix = "hexadecimal";
            }
            SIGNAL acb
            {
               format = "Logic";
               name = "M_en";
               radix = "hexadecimal";
            }
            SIGNAL acc
            {
               format = "Logic";
               name = "A_en";
               radix = "hexadecimal";
            }
            SIGNAL acd
            {
               format = "Logic";
               name = "F_iw";
               radix = "hexadecimal";
            }
            SIGNAL ace
            {
               format = "Logic";
               name = "D_iw";
               radix = "hexadecimal";
            }
            SIGNAL acf
            {
               format = "Logic";
               name = "E_iw";
               radix = "hexadecimal";
            }
            SIGNAL acg
            {
               format = "Logic";
               name = "M_pipe_flush";
               radix = "hexadecimal";
            }
            SIGNAL ach
            {
               format = "Logic";
               name = "M_pipe_flush_baddr";
               radix = "hexadecimal";
            }
            SIGNAL aci
            {
               format = "Logic";
               name = "norm_intr_req";
               radix = "hexadecimal";
            }
            SIGNAL acj
            {
               format = "Logic";
               name = "A_status_reg";
               radix = "hexadecimal";
            }
            SIGNAL ack
            {
               format = "Logic";
               name = "A_status_reg_pie";
               radix = "hexadecimal";
            }
            SIGNAL acl
            {
               format = "Logic";
               name = "A_estatus_reg";
               radix = "hexadecimal";
            }
            SIGNAL acm
            {
               format = "Logic";
               name = "A_estatus_reg_pie";
               radix = "hexadecimal";
            }
            SIGNAL acn
            {
               format = "Logic";
               name = "A_bstatus_reg";
               radix = "hexadecimal";
            }
            SIGNAL aco
            {
               format = "Logic";
               name = "A_bstatus_reg_pie";
               radix = "hexadecimal";
            }
            SIGNAL acp
            {
               format = "Logic";
               name = "A_ienable_reg";
               radix = "hexadecimal";
            }
            SIGNAL acq
            {
               format = "Logic";
               name = "A_ienable_reg_irq0";
               radix = "hexadecimal";
            }
            SIGNAL acr
            {
               format = "Logic";
               name = "A_ipending_reg";
               radix = "hexadecimal";
            }
            SIGNAL acs
            {
               format = "Logic";
               name = "A_ipending_reg_irq0";
               radix = "hexadecimal";
            }
            SIGNAL act
            {
               format = "Logic";
               name = "A_cpuid_reg";
               radix = "hexadecimal";
            }
            SIGNAL acu
            {
               format = "Logic";
               name = "E_valid_prior_to_hbreak";
               radix = "hexadecimal";
            }
         }
      }
   }
   MODULE jtag_uart
   {
      SLAVE avalon_jtag_slave
      {
         PORT_WIRING 
         {
            PORT clk
            {
               type = "clk";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT rst_n
            {
               type = "reset_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT av_irq
            {
               type = "irq";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT av_chipselect
            {
               type = "chipselect";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT av_address
            {
               type = "address";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT av_read_n
            {
               type = "read_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT av_readdata
            {
               type = "readdata";
               width = "32";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT av_write_n
            {
               type = "write_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT av_writedata
            {
               type = "writedata";
               width = "32";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT av_waitrequest
            {
               type = "waitrequest";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT dataavailable
            {
               type = "dataavailable";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT readyfordata
            {
               type = "readyfordata";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Has_IRQ = "1";
            Bus_Type = "avalon";
            Read_Wait_States = "peripheral_controlled";
            Write_Wait_States = "peripheral_controlled";
            Hold_Time = "0cycles";
            Setup_Time = "0cycles";
            Is_Printable_Device = "1";
            Address_Alignment = "native";
            Well_Behaved_Waitrequest = "0";
            Is_Nonvolatile_Storage = "0";
            Read_Latency = "0";
            Is_Memory_Device = "0";
            Maximum_Pending_Read_Transactions = "0";
            Minimum_Uninterrupted_Run_Length = "1";
            Accepts_Internal_Connections = "1";
            Write_Latency = "0";
            Is_Flash = "0";
            Data_Width = "32";
            Address_Width = "1";
            Maximum_Burst_Size = "1";
            Register_Incoming_Signals = "0";
            Register_Outgoing_Signals = "0";
            Interleave_Bursts = "0";
            Linewrap_Bursts = "0";
            Burst_On_Burst_Boundaries_Only = "0";
            Always_Burst_Max_Burst = "0";
            Is_Big_Endian = "0";
            Is_Enabled = "1";
            JTAG_Hub_Base_Id = "262254";
            JTAG_Hub_Instance_Id = "0";
            Connection_Limit = "1";
            MASTERED_BY cpu/data_master
            {
               priority = "1";
               Offset_Address = "0x00011010";
            }
            IRQ_MASTER cpu/data_master
            {
               IRQ_Number = "0";
            }
            Base_Address = "0x00011010";
            Address_Group = "0";
         }
      }
      class = "altera_avalon_jtag_uart";
      class_version = "7.08101";
      iss_model_name = "altera_avalon_jtag_uart";
      WIZARD_SCRIPT_ARGUMENTS 
      {
         write_depth = "64";
         read_depth = "64";
         write_threshold = "8";
         read_threshold = "8";
         read_char_stream = "";
         showascii = "1";
         relativepath = "1";
         read_le = "0";
         write_le = "0";
         altera_show_unreleased_jtag_uart_features = "0";
      }
      SIMULATION 
      {
         DISPLAY 
         {
            SIGNAL av_chipselect
            {
               name = "av_chipselect";
            }
            SIGNAL av_address
            {
               name = "av_address";
               radix = "hexadecimal";
            }
            SIGNAL av_read_n
            {
               name = "av_read_n";
            }
            SIGNAL av_readdata
            {
               name = "av_readdata";
               radix = "hexadecimal";
            }
            SIGNAL av_write_n
            {
               name = "av_write_n";
            }
            SIGNAL av_writedata
            {
               name = "av_writedata";
               radix = "hexadecimal";
            }
            SIGNAL av_waitrequest
            {
               name = "av_waitrequest";
            }
            SIGNAL dataavailable
            {
               name = "dataavailable";
            }
            SIGNAL readyfordata
            {
               name = "readyfordata";
            }
            SIGNAL av_irq
            {
               name = "av_irq";
            }
         }
         INTERACTIVE_IN drive
         {
            enable = "0";
            file = "_input_data_stream.dat";
            mutex = "_input_data_mutex.dat";
            log = "_in.log";
            rate = "100";
            signals = "temp,list";
            exe = "nios2-terminal";
         }
         INTERACTIVE_OUT log
         {
            enable = "1";
            exe = "perl -- atail-f.pl";
            file = "_output_stream.dat";
            radix = "ascii";
            signals = "temp,list";
         }
         Fix_Me_Up = "";
      }
      SYSTEM_BUILDER_INFO 
      {
         Is_Enabled = "1";
         Clock_Source = "clk_50";
         Has_Clock = "1";
         Instantiate_In_System_Module = "1";
         Iss_Launch_Telnet = "0";
         Top_Level_Ports_Are_Enumerated = "1";
         View 
         {
            MESSAGES 
            {
            }
            Settings_Summary = "<br>Write Depth: 64; Write IRQ Threshold: 8
                <br>Read  Depth: 64; Read  IRQ Threshold: 8";
         }
      }
      HDL_INFO 
      {
         Precompiled_Simulation_Library_Files = "";
         Simulation_HDL_Files = "";
         Synthesis_HDL_Files = "__PROJECT_DIRECTORY__/jtag_uart.v";
         Synthesis_Only_Files = "";
      }
      PORT_WIRING 
      {
      }
   }
   MODULE onchip_memory2
   {
      SLAVE s1
      {
         PORT_WIRING 
         {
            PORT clk
            {
               type = "clk";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT reset
            {
               type = "reset";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT address
            {
               type = "address";
               width = "13";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT chipselect
            {
               type = "chipselect";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT clken
            {
               type = "clken";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
               default_value = "1'b1";
            }
            PORT readdata
            {
               type = "readdata";
               width = "32";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT write
            {
               type = "write";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT writedata
            {
               type = "writedata";
               width = "32";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT byteenable
            {
               type = "byteenable";
               width = "4";
               direction = "input";
               Is_Enabled = "1";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Write_Wait_States = "0cycles";
            Read_Wait_States = "0cycles";
            Hold_Time = "0cycles";
            Setup_Time = "0cycles";
            Is_Printable_Device = "0";
            Address_Alignment = "dynamic";
            Well_Behaved_Waitrequest = "0";
            Is_Nonvolatile_Storage = "0";
            Address_Span = "26000";
            Read_Latency = "1";
            Is_Memory_Device = "1";
            Maximum_Pending_Read_Transactions = "0";
            Minimum_Uninterrupted_Run_Length = "1";
            Accepts_Internal_Connections = "1";
            Write_Latency = "0";
            Is_Flash = "0";
            Data_Width = "32";
            Address_Width = "13";
            Maximum_Burst_Size = "1";
            Register_Incoming_Signals = "0";
            Register_Outgoing_Signals = "0";
            Interleave_Bursts = "0";
            Linewrap_Bursts = "0";
            Burst_On_Burst_Boundaries_Only = "0";
            Always_Burst_Max_Burst = "0";
            Is_Big_Endian = "0";
            Is_Enabled = "1";
            MASTERED_BY cpu/instruction_master
            {
               priority = "1";
               Offset_Address = "0x00008000";
            }
            MASTERED_BY cpu/data_master
            {
               priority = "1";
               Offset_Address = "0x00008000";
            }
            Base_Address = "0x00008000";
            Address_Group = "0";
            Has_IRQ = "0";
            Is_Channel = "1";
            Is_Writable = "1";
            IRQ_MASTER cpu/data_master
            {
               IRQ_Number = "NC";
            }
         }
      }
      iss_model_name = "altera_memory";
      WIZARD_SCRIPT_ARGUMENTS 
      {
         allow_mram_sim_contents_only_file = "0";
         ram_block_type = "AUTO";
         init_contents_file = "onchip_memory2";
         non_default_init_file_enabled = "0";
         gui_ram_block_type = "Automatic";
         Writeable = "1";
         dual_port = "0";
         Size_Value = "26000";
         Size_Multiple = "1";
         use_shallow_mem_blocks = "0";
         init_mem_content = "1";
         allow_in_system_memory_content_editor = "0";
         instance_id = "NONE";
         read_during_write_mode = "DONT_CARE";
         ignore_auto_block_type_assignment = "1";
         MAKE 
         {
            TARGET delete_placeholder_warning
            {
               onchip_memory2 
               {
                  Command1 = "rm -f $(SIMDIR)/contents_file_warning.txt";
                  Is_Phony = "1";
                  Target_File = "do_delete_placeholder_warning";
               }
            }
            TARGET hex
            {
               onchip_memory2 
               {
                  Command1 = "@echo Post-processing to create $(notdir $@)";
                  Command2 = "elf2hex $(ELF) 0x00008000 0xE58F --width=32 $(QUARTUS_PROJECT_DIR)/onchip_memory2.hex --create-lanes=0 ";
                  Dependency = "$(ELF)";
                  Target_File = "$(QUARTUS_PROJECT_DIR)/onchip_memory2.hex";
               }
            }
            TARGET sim
            {
               onchip_memory2 
               {
                  Command1 = "if [ ! -d $(SIMDIR) ]; then mkdir $(SIMDIR) ; fi";
                  Command2 = "@echo Hardware simulation is not enabled for the target SOPC Builder system. Skipping creation of hardware simulation model contents and simulation symbol files. \\(Note: This does not affect the instruction set simulator.\\)";
                  Command3 = "touch $(SIMDIR)/dummy_file";
                  Dependency = "$(ELF)";
                  Target_File = "$(SIMDIR)/dummy_file";
               }
            }
         }
         contents_info = "QUARTUS_PROJECT_DIR/onchip_memory2.hex 1298291149 ";
      }
      SIMULATION 
      {
         DISPLAY 
         {
            SIGNAL a
            {
               name = "chipselect";
               conditional = "1";
            }
            SIGNAL c
            {
               name = "address";
               radix = "hexadecimal";
            }
            SIGNAL d
            {
               name = "byteenable";
               radix = "binary";
               conditional = "1";
            }
            SIGNAL e
            {
               name = "readdata";
               radix = "hexadecimal";
            }
            SIGNAL b
            {
               name = "write";
               conditional = "1";
            }
            SIGNAL f
            {
               name = "writedata";
               radix = "hexadecimal";
               conditional = "1";
            }
         }
      }
      SYSTEM_BUILDER_INFO 
      {
         Prohibited_Device_Family = "MERCURY, APEX20K, APEX20KE, APEX20KC, APEXII, ACEX1K, FLEX10KE, EXCALIBUR_ARM, MAXII";
         Instantiate_In_System_Module = "1";
         Is_Enabled = "1";
         Default_Module_Name = "onchip_memory";
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk_50";
         Has_Clock = "1";
         View 
         {
            MESSAGES 
            {
            }
         }
      }
      class = "altera_avalon_onchip_memory2";
      class_version = "7.08101";
      HDL_INFO 
      {
         Precompiled_Simulation_Library_Files = "";
         Simulation_HDL_Files = "";
         Synthesis_HDL_Files = "__PROJECT_DIRECTORY__/onchip_memory2.v";
         Synthesis_Only_Files = "";
      }
      SLAVE s2
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Is_Memory_Device = "1";
            Address_Group = "0";
            Address_Alignment = "dynamic";
            Address_Width = "13";
            Data_Width = "32";
            Has_IRQ = "0";
            Read_Wait_States = "0";
            Write_Wait_States = "0";
            Address_Span = "26000";
            Read_Latency = "1";
            Is_Channel = "1";
            Is_Enabled = "0";
            Is_Writable = "1";
         }
      }
      PORT_WIRING 
      {
      }
   }
   MODULE pio_led
   {
      SLAVE s1
      {
         PORT_WIRING 
         {
            PORT clk
            {
               type = "clk";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT reset_n
            {
               type = "reset_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT address
            {
               type = "address";
               width = "2";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT write_n
            {
               type = "write_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT writedata
            {
               type = "writedata";
               width = "8";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT chipselect
            {
               type = "chipselect";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT readdata
            {
               type = "readdata";
               width = "8";
               direction = "output";
               Is_Enabled = "1";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Write_Wait_States = "0cycles";
            Read_Wait_States = "1cycles";
            Hold_Time = "0cycles";
            Setup_Time = "0cycles";
            Is_Printable_Device = "0";
            Address_Alignment = "native";
            Well_Behaved_Waitrequest = "0";
            Is_Nonvolatile_Storage = "0";
            Read_Latency = "0";
            Is_Memory_Device = "0";
            Maximum_Pending_Read_Transactions = "0";
            Minimum_Uninterrupted_Run_Length = "1";
            Accepts_Internal_Connections = "1";
            Write_Latency = "0";
            Is_Flash = "0";
            Data_Width = "8";
            Address_Width = "2";
            Maximum_Burst_Size = "1";
            Register_Incoming_Signals = "0";
            Register_Outgoing_Signals = "0";
            Interleave_Bursts = "0";
            Linewrap_Bursts = "0";
            Burst_On_Burst_Boundaries_Only = "0";
            Always_Burst_Max_Burst = "0";
            Is_Big_Endian = "0";
            Is_Enabled = "1";
            MASTERED_BY cpu/data_master
            {
               priority = "1";
               Offset_Address = "0x00011000";
            }
            Base_Address = "0x00011000";
            Has_IRQ = "0";
            Address_Group = "0";
            IRQ_MASTER cpu/data_master
            {
               IRQ_Number = "NC";
            }
            Is_Readable = "0";
            Is_Writable = "1";
         }
      }
      PORT_WIRING 
      {
         PORT out_port
         {
            type = "export";
            width = "8";
            direction = "output";
            Is_Enabled = "1";
         }
         PORT in_port
         {
            direction = "input";
            Is_Enabled = "0";
            width = "8";
         }
         PORT bidir_port
         {
            direction = "inout";
            Is_Enabled = "0";
            width = "8";
         }
      }
      class = "altera_avalon_pio";
      class_version = "7.08101";
      SYSTEM_BUILDER_INFO 
      {
         Is_Enabled = "1";
         Instantiate_In_System_Module = "1";
         Wire_Test_Bench_Values = "1";
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk_50";
         Has_Clock = "1";
         Date_Modified = "";
         View 
         {
            MESSAGES 
            {
            }
            Settings_Summary = " 8-bit PIO using <br>
					
					
					 output pins";
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         Do_Test_Bench_Wiring = "0";
         Driven_Sim_Value = "0";
         has_tri = "0";
         has_out = "1";
         has_in = "0";
         capture = "0";
         Data_Width = "8";
         reset_value = "0";
         edge_type = "NONE";
         irq_type = "NONE";
         bit_clearing_edge_register = "0";
         bit_modifying_output_register = "0";
      }
      HDL_INFO 
      {
         Precompiled_Simulation_Library_Files = "";
         Simulation_HDL_Files = "";
         Synthesis_HDL_Files = "__PROJECT_DIRECTORY__/pio_led.v";
         Synthesis_Only_Files = "";
      }
   }
}
